//
// NopSCADlib Copyright Chris Palmer 2018
// nop.head@gmail.com
// hydraraptor.blogspot.com
//
// This file is part of NopSCADlib.
//
// NopSCADlib is free software: you can redistribute it and/or modify it under the terms of the
// GNU General Public License as published by the Free Software Foundation, either version 3 of
// the License, or (at your option) any later version.
//
// NopSCADlib is distributed in the hope that it will be useful, but WITHOUT ANY WARRANTY;
// without even the implied warranty of MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.
// See the GNU General Public License for more details.
//
// You should have received a copy of the GNU General Public License along with NopSCADlib.
// If not, see <https://www.gnu.org/licenses/>.
//

//
// Microswitches
//
small_leg  = [0.9,  3.3, 0.4, 0];
medium_leg = [0.5,  3.9, 3.2, 1.6, [0, -0.5]];
large_leg  = [11.4, 0.8, 6.3, 1.8, [1.7, 0]];

small_microswitch  = ["small_microswitch", "DM1-00P-110-3",      5.8, 6.5,  12.8, 0, 2,    [[-3.25, -1.65], [3.25, -1.65]], 2.9, 1.2, [-1.95, 3.75], [[-5.08, -4.95], [0,    -4.9],  [5.08, -4.9]  ], small_leg,  grey20, "white"  ];
medium_microswitch = ["medium_microswitch","SS-01 or SS-5GL",    6.4, 10.2, 19.8, 1, 2.35, [[-4.8,  -2.6 ], [4.7,  -2.6 ]], 3.2, 2,   [-2.8,  5.8 ], [[-8.05, -7.05], [0.75, -7.05], [8.05, -7.05] ], medium_leg, grey20, "burlywood" ];
large_microswitch  = ["large_microswitch", "Saia G3 low force", 10.4, 15.9, 28.0, 2, 3.1,  [[-11.1, -5.15], [11.2,  5.15]], 4,   2.75,[-9.1,  9.55], [[19.7,   2.19], [19.7, -3.45],  [8.3, -10.45] ], large_leg,  "ivory", "white" ];

microswitches = [small_microswitch, medium_microswitch, large_microswitch];

use <microswitch.scad>
