//
// NopSCADlib Copyright Chris Palmer 2018
// nop.head@gmail.com
// hydraraptor.blogspot.com
//
// This file is part of NopSCADlib.
//
// NopSCADlib is free software: you can redistribute it and/or modify it under the terms of the
// GNU General Public License as published by the Free Software Foundation, either version 3 of
// the License, or (at your option) any later version.
//
// NopSCADlib is distributed in the hope that it will be useful, but WITHOUT ANY WARRANTY;
// without even the implied warranty of MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.
// See the GNU General Public License for more details.
//
// You should have received a copy of the GNU General Public License along with NopSCADlib.
// If not, see <https://www.gnu.org/licenses/>.
//

include <spades.scad>

small_spades = [[spade4p8, 7.6, 0, 0,   0],
                [spade4p8, 7.6, 0, 7.1, 0]];

neon_spades  = [[spade4p8, 7.3, 0, -7, 0],
                [spade4p8, 7.3, 0,  7, 0]];

//
//                                   p                                 s   s     f   f   f  w     h     d     b    p    b
//                                   a                                 l   l     l   l   l  i     e     e     e    i    u
//                                   r                                 o   o     a   a   a  d     i     p     z    v    t
//                                   t                                 t   t     n   n   n  t     g     t     e    o    t
//                                                                               g   g   g  h     h     h     l    t    o
//                                                                     w   h     e   e   e        t                     n
//
//                                                                               w   h   t
//
small_rocker   = ["small_rocker",   "Rocker Switch PRASA1-16F-BB0BW", 13, 19.8, 15, 21, 2, 12.8, 18.5, 11.8, 2.5,  -1, 3.8, small_spades];
neon_indicator = ["neon_indicator", "Neon Indicator H8630FBNAL",      13, 19.8, 15, 21, 2, 12.8, 18.5, 12.5, 2.5,  0,  0.3, neon_spades];

rockers = [small_rocker, neon_indicator];

use <rocker.scad>
